Give distinct step by step instructions on how to operate the Konexial My20 ELD IOS version to log in and start operating a vehicle.

To operate the Konexial My20 ELD (Electronic Logging Device) on an iOS device, follow these steps to log in and start operating a vehicle:

**Step 1: Download the Konexial My20 App**

1. Open the **App Store** on your iOS device.
2. Search for **Konexial My20** in the search bar.
3. Download and install the app onto your device.

**Step 2: Launch the App**

1. Locate the **Konexial My20** app icon on your home screen.
2. Tap on the icon to open the app.

**Step 3: Log In to the App**

1. When the app opens, you’ll be prompted to **enter your login credentials** (username and password).
   * If you don't have an account, follow the instructions for registration. You’ll typically need your company’s information or a specific registration code from your fleet manager.
2. Once entered, tap the **Login** button.

**Step 4: Allow Permissions**

1. Upon first-time login, you may be prompted to allow the app to access certain features on your device (such as location services, notifications, etc.).
2. **Grant the necessary permissions** for the app to function properly.

**Step 5: Connect to the Vehicle**

1. Ensure that the vehicle is powered on.
2. The app should automatically detect your vehicle’s ELD if the vehicle’s telematics system is connected.
   * If the system doesn’t connect automatically, you might be asked to pair via Bluetooth or enter the vehicle’s unique identifier (VIN or other details).
3. Once connected, your vehicle’s information should appear on the screen.

**Step 6: Select Driver Profile**

1. Choose your **driver profile** from the list (this should appear after login, or you may be prompted to create one).
2. Make sure your **driver ID** and other information are correctly displayed.
   * If you have multiple drivers for a vehicle, you can switch between profiles as necessary.

**Step 7: Confirm Pre-Trip Inspection**

1. Before starting the vehicle, the app will prompt you to conduct a **pre-trip inspection**.
2. Follow the on-screen instructions to verify that you’ve completed the necessary checks for the vehicle (e.g., lights, tires, brakes, etc.).
3. Once the inspection is completed, mark it as **completed** or **pass**.

**Step 8: Start the Vehicle and Begin Driving**

1. After completing the pre-trip inspection, you should see an option to **start driving**.
2. Tap **Start** or **Drive** to begin recording your driving hours.
3. The app will automatically start logging your driving time and tracking your vehicle's movements via GPS.
   * Your status will change from **On Duty** to **Driving** as soon as the vehicle starts moving.

**Step 9: Monitor Your Hours and Status**

1. The app will continuously track your **HOS (Hours of Service)** and show your current duty status.
2. You can also view your remaining drive time, breaks, and duty cycles.

**Step 10: Log Out or Change Status After Driving**

1. Once you stop driving and complete the trip, you can **change your status** to Off Duty, On Duty, or Sleep.
2. Ensure that the app is updated with your accurate status for compliance.

**Troubleshooting Tips:**

* **Bluetooth Connection Issues:** If the app is not connecting to the vehicle, make sure Bluetooth is enabled on your iOS device and check that your vehicle's ELD is powered on.
* **App Not Detecting Vehicle:** Try restarting the app or the vehicle’s ELD system, and check if the app requires any updates.
* **Location Issues:** If the GPS isn't tracking your route, ensure location services are turned on for the app.

By following these steps, you should be able to successfully log in, connect to your vehicle, and start using the Konexial My20 ELD app to record your driving activity.